<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="40" width="0" layer="20"/>
<wire x1="50" y1="40" x2="0" y2="40" width="0" layer="20"/>
<wire x1="0" y1="40" x2="0" y2="0" width="0" layer="20"/>
<wire x1="76.2" y1="66.04" x2="0" y2="66.04" width="0" layer="20"/>
<wire x1="0" y1="66.04" x2="0" y2="43.18" width="0" layer="20"/>
<wire x1="76.2" y1="66.04" x2="76.2" y2="43.18" width="0" layer="20"/>
<wire x1="76.2" y1="43.18" x2="0" y2="43.18" width="0" layer="20"/>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
</packages>
</library>
<library name="con-lstb">
<packages>
<package name="MA12-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO34Z7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 1.8 mm, horizontal, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="con-berg">
<packages>
<package name="PN61729-S">
<description>&lt;b&gt;USB connector&lt;/b&gt; with shield&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="f0086">
<packages>
<package name="SMD">
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="SO20L$">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, large</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="rcl" package="0204V" value="10k"/>
<element name="LED1" library="led" package="LED5MM" value=""/>
<element name="LED2" library="led" package="LED5MM" value=""/>
<element name="LED3" library="led" package="LED5MM" value=""/>
<element name="LED6" library="led" package="LED5MM" value=""/>
<element name="LED5" library="led" package="LED5MM" value=""/>
<element name="LED4" library="led" package="LED5MM" value=""/>
<element name="LED7" library="led" package="LED5MM" value=""/>
<element name="LED8" library="led" package="LED5MM" value=""/>
<element name="LED9" library="led" package="LED5MM" value=""/>
<element name="C3" library="rcl" package="C025-024X044" value="100n"/>
<element name="LED16" library="led" package="LED5MM" value=""/>
<element name="LED17" library="led" package="LED5MM" value=""/>
<element name="LED18" library="led" package="LED5MM" value=""/>
<element name="LED24" library="led" package="LED5MM" value=""/>
<element name="LED23" library="led" package="LED5MM" value=""/>
<element name="LED22" library="led" package="LED5MM" value=""/>
<element name="LED25" library="led" package="LED5MM" value=""/>
<element name="LED26" library="led" package="LED5MM" value=""/>
<element name="LED27" library="led" package="LED5MM" value=""/>
<element name="LED10" library="led" package="LED5MM" value=""/>
<element name="LED11" library="led" package="LED5MM" value=""/>
<element name="LED12" library="led" package="LED5MM" value=""/>
<element name="LED15" library="led" package="LED5MM" value=""/>
<element name="LED14" library="led" package="LED5MM" value=""/>
<element name="LED13" library="led" package="LED5MM" value=""/>
<element name="LED19" library="led" package="LED5MM" value=""/>
<element name="LED20" library="led" package="LED5MM" value=""/>
<element name="LED21" library="led" package="LED5MM" value=""/>
<element name="Q1" library="crystal" package="HC49/S" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="C1" library="rcl" package="C025-024X044" value="27p"/>
<element name="C2" library="rcl" package="C025-024X044" value="27p"/>
<element name="R3" library="rcl" package="0204V" value="69"/>
<element name="R4" library="rcl" package="0204V" value="69"/>
<element name="R2" library="rcl" package="0204V" value="1k5"/>
<element name="D1" library="diode" package="DO34Z7" value="3V6"/>
<element name="D2" library="diode" package="DO34Z7" value="3V6"/>
<element name="X1" library="con-berg" package="PN61729-S" value="USB">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="SV6" library="con-lstb" package="MA12-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="ISP1" library="f0086" package="SMD" value="SMD-ISP"/>
<element name="U$1" library="avr-7" package="SO20L$" value="TINY2313-*S*"/>
</elements>
<signals>
<signal name="+5V">
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="ISP1" pad="VCC"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="A"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="S1"/>
<contactref element="X1" pad="S2"/>
<contactref element="ISP1" pad="GND"/>
<contactref element="U$1" pad="10"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="A">
<contactref element="SV6" pad="10"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="B">
<contactref element="SV6" pad="11"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="C">
<contactref element="SV6" pad="12"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="9">
<contactref element="SV6" pad="9"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="1">
<contactref element="SV6" pad="1"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="2">
<contactref element="SV6" pad="2"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="3">
<contactref element="SV6" pad="3"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="4">
<contactref element="SV6" pad="4"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="5">
<contactref element="SV6" pad="5"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="6_MOSI">
<contactref element="SV6" pad="6"/>
<contactref element="ISP1" pad="MOSI"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="7_MISO">
<contactref element="SV6" pad="7"/>
<contactref element="ISP1" pad="MISO"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="8_SCK">
<contactref element="SV6" pad="8"/>
<contactref element="ISP1" pad="SCK"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="D+">
<contactref element="R3" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="D-">
<contactref element="R4" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="X1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="C_">
<contactref element="LED3" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED12" pad="A"/>
<contactref element="LED10" pad="A"/>
<contactref element="LED11" pad="A"/>
<contactref element="LED18" pad="A"/>
<contactref element="LED16" pad="A"/>
<contactref element="LED17" pad="A"/>
</signal>
<signal name="B_">
<contactref element="LED6" pad="A"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED24" pad="A"/>
<contactref element="LED23" pad="A"/>
<contactref element="LED22" pad="A"/>
<contactref element="LED15" pad="A"/>
<contactref element="LED14" pad="A"/>
<contactref element="LED13" pad="A"/>
</signal>
<signal name="A_">
<contactref element="LED9" pad="A"/>
<contactref element="LED8" pad="A"/>
<contactref element="LED7" pad="A"/>
<contactref element="LED27" pad="A"/>
<contactref element="LED26" pad="A"/>
<contactref element="LED25" pad="A"/>
<contactref element="LED21" pad="A"/>
<contactref element="LED20" pad="A"/>
<contactref element="LED19" pad="A"/>
</signal>
<signal name="1_">
<contactref element="LED4" pad="K"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED7" pad="K"/>
</signal>
<signal name="2_">
<contactref element="LED5" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED8" pad="K"/>
</signal>
<signal name="3_">
<contactref element="LED3" pad="K"/>
<contactref element="LED6" pad="K"/>
<contactref element="LED9" pad="K"/>
</signal>
<signal name="9_">
<contactref element="LED12" pad="K"/>
<contactref element="LED15" pad="K"/>
<contactref element="LED21" pad="K"/>
</signal>
<signal name="8_SCK_">
<contactref element="LED14" pad="K"/>
<contactref element="LED11" pad="K"/>
<contactref element="LED20" pad="K"/>
</signal>
<signal name="7_MISO_">
<contactref element="LED13" pad="K"/>
<contactref element="LED10" pad="K"/>
<contactref element="LED19" pad="K"/>
</signal>
<signal name="6_MOSI_">
<contactref element="LED18" pad="K"/>
<contactref element="LED24" pad="K"/>
<contactref element="LED27" pad="K"/>
</signal>
<signal name="5_">
<contactref element="LED23" pad="K"/>
<contactref element="LED17" pad="K"/>
<contactref element="LED26" pad="K"/>
</signal>
<signal name="4_">
<contactref element="LED22" pad="K"/>
<contactref element="LED16" pad="K"/>
<contactref element="LED25" pad="K"/>
</signal>
<signal name="N$6">
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="ISP1" pad="RESET"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="6"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
