(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-2~bpo8+1-stable)

  (general
    (links 55)
    (no_connects 0)
    (area 78.05188 66.6095 138.331334 151.666333)
    (thickness 1.6)
    (drawings 0)
    (tracks 198)
    (zones 0)
    (modules 28)
    (nets 42)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 /CLK0)
  (net 7 "Net-(C4-Pad2)")
  (net 8 "Net-(C5-Pad2)")
  (net 9 +5V)
  (net 10 "Net-(C7-Pad1)")
  (net 11 "Net-(D1-Pad2)")
  (net 12 /A0)
  (net 13 /A1)
  (net 14 "Net-(P3-Pad1)")
  (net 15 "Net-(P3-Pad2)")
  (net 16 "Net-(P3-Pad3)")
  (net 17 "Net-(P3-Pad5)")
  (net 18 "Net-(P3-Pad6)")
  (net 19 "Net-(P3-Pad7)")
  (net 20 "Net-(P3-Pad8)")
  (net 21 "Net-(P3-Pad9)")
  (net 22 "Net-(P3-Pad10)")
  (net 23 "Net-(P3-Pad11)")
  (net 24 "Net-(P3-Pad12)")
  (net 25 "Net-(P3-Pad13)")
  (net 26 "Net-(P3-Pad14)")
  (net 27 "Net-(P3-Pad15)")
  (net 28 /CLK1)
  (net 29 /CLK2)
  (net 30 /SCL)
  (net 31 /SDA)
  (net 32 "Net-(P5-Pad1)")
  (net 33 /RESET)
  (net 34 "Net-(P5-Pad5)")
  (net 35 "Net-(P5-Pad6)")
  (net 36 "Net-(P5-Pad9)")
  (net 37 "Net-(P5-Pad10)")
  (net 38 "Net-(P5-Pad14)")
  (net 39 "Net-(P5-Pad15)")
  (net 40 "Net-(R1-Pad1)")
  (net 41 "Net-(R5-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /CLK0)
    (add_net /CLK1)
    (add_net /CLK2)
    (add_net /RESET)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad11)")
    (add_net "Net-(P3-Pad12)")
    (add_net "Net-(P3-Pad13)")
    (add_net "Net-(P3-Pad14)")
    (add_net "Net-(P3-Pad15)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P3-Pad9)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad10)")
    (add_net "Net-(P5-Pad14)")
    (add_net "Net-(P5-Pad15)")
    (add_net "Net-(P5-Pad5)")
    (add_net "Net-(P5-Pad6)")
    (add_net "Net-(P5-Pad9)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R5-Pad1)")
  )

  (module Connect:PINHEAD1-3 (layer F.Cu) (tedit 57DD8681) (tstamp 57DD845A)
    (at 93.726 72.898)
    (path /57D82265)
    (attr virtual)
    (fp_text reference P1 (at 0.05 -3.8) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BNC (at 0 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -3.175) (end -3.81 3.175) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 -3.175) (end 3.81 3.175) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 -1.27) (end -3.81 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.81 -3.175) (end 3.81 -3.175) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 3.175) (end -3.81 3.175) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole oval (at 0 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask))
  )

  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0) (tstamp 57DD82BE)
    (at 84.328 110.49)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (path /57D8211D)
    (fp_text reference C1 (at 1.25 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10n (at 1.25 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.9 -1.5) (end 3.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 -1.5) (end 3.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 1.5) (end -0.9 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 1.5) (end -0.9 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.25 -1.25) (end 2.75 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.75 1.25) (end -0.25 1.25) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0) (tstamp 57DD82C4)
    (at 105.537 75.057 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (path /57D81D90)
    (fp_text reference C2 (at 1.25 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.9 -1.5) (end 3.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 -1.5) (end 3.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 1.5) (end -0.9 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 1.5) (end -0.9 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.25 -1.25) (end 2.75 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.75 1.25) (end -0.25 1.25) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0) (tstamp 57DD82CA)
    (at 96.774 110.49)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (path /57D821F7)
    (fp_text reference C3 (at 1.25 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10n (at 1.25 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.9 -1.5) (end 3.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 -1.5) (end 3.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 1.5) (end -0.9 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 1.5) (end -0.9 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.25 -1.25) (end 2.75 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.75 1.25) (end -0.25 1.25) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0) (tstamp 57DD82D0)
    (at 118.554 72.8345 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (path /57D81AA8)
    (fp_text reference C4 (at 1.25 -2.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.9 -1.5) (end 3.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 -1.5) (end 3.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 1.5) (end -0.9 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 1.5) (end -0.9 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.25 -1.25) (end 2.75 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.75 1.25) (end -0.25 1.25) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /CLK0))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C4-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0) (tstamp 57DD82D6)
    (at 118.872 96.647 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (path /57D82040)
    (fp_text reference C5 (at 1.25 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.9 -1.5) (end 3.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 -1.5) (end 3.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 1.5) (end -0.9 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 1.5) (end -0.9 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.25 -1.25) (end 2.75 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.75 1.25) (end -0.25 1.25) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0) (tstamp 57DD82DC)
    (at 117.666 85.6615 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (path /57D85D32)
    (fp_text reference C6 (at 1.25 -2.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.9 -1.5) (end 3.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 -1.5) (end 3.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 1.5) (end -0.9 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 1.5) (end -0.9 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.25 -1.25) (end 2.75 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.75 1.25) (end -0.25 1.25) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0) (tstamp 57DD82E2)
    (at 129.159 143.891 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (path /57D87F1E)
    (fp_text reference C7 (at 1.25 -2.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.9 -1.5) (end 3.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 -1.5) (end 3.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.4 1.5) (end -0.9 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 1.5) (end -0.9 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.25 -1.25) (end 2.75 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.75 1.25) (end -0.25 1.25) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 552FFC30) (tstamp 57DD82E8)
    (at 86.614 89.535)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (path /57D81E7A)
    (fp_text reference D1 (at 5.43052 2.53746) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1N60 (at 4.41452 -3.55854) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.36652 -0.00254) (end 8.76352 -0.00254) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.92152 -0.00254) (end 1.39752 -0.00254) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.30252 -0.76454) (end 3.30252 0.75946) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.04852 -0.76454) (end 3.04852 0.75946) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.79452 -0.00254) (end 2.79452 0.75946) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.79452 0.75946) (end 7.36652 0.75946) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.36652 0.75946) (end 7.36652 -0.76454) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.36652 -0.76454) (end 2.79452 -0.76454) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.79452 -0.76454) (end 2.79452 -0.00254) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )

  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 552FFC30) (tstamp 57DD82EE)
    (at 111.252 89.535 180)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (path /57D81FC0)
    (fp_text reference D2 (at 5.43052 2.53746 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1N60 (at 4.41452 -3.55854 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.36652 -0.00254) (end 8.76352 -0.00254) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.92152 -0.00254) (end 1.39752 -0.00254) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.30252 -0.76454) (end 3.30252 0.75946) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.04852 -0.76454) (end 3.04852 0.75946) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.79452 -0.00254) (end 2.79452 0.75946) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.79452 0.75946) (end 7.36652 0.75946) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.36652 0.75946) (end 7.36652 -0.76454) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.36652 -0.76454) (end 2.79452 -0.76454) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.79452 -0.76454) (end 2.79452 -0.00254) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at 10.16052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD833A)
    (at 82.677 131.953 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D817F0)
    (fp_text reference R1 (at 5.32892 -3.50012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 680 (at 5.08 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 40 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD8340)
    (at 82.677 146.431 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D8194B)
    (fp_text reference R2 (at 5.32892 -3.50012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 6k8 (at 5.08 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 /A1))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 40 "Net-(R1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD8346)
    (at 92.456 116.078 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D81651)
    (fp_text reference R3 (at 5.32892 -3.50012 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 5.08 3.81 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD834C)
    (at 86.741 104.394 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D8156D)
    (fp_text reference R4 (at 5.32892 -3.50012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 5.08 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD8352)
    (at 106.68 131.953 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D81862)
    (fp_text reference R5 (at 5.32892 -3.50012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 680 (at 5.08 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 41 "Net-(R5-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD8358)
    (at 106.68 146.431 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D818FD)
    (fp_text reference R6 (at 5.32892 -3.50012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 6k8 (at 5.08 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 /A0))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 41 "Net-(R5-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD835E)
    (at 112.204 82.7405 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D81418)
    (fp_text reference R7 (at 5.32892 -3.50012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at 5.08 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD8364)
    (at 106.934 116.078 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D81777)
    (fp_text reference R8 (at 5.32892 -3.50012 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 5.08 3.81 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD836A)
    (at 96.9645 82.7405)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D814B0)
    (fp_text reference R9 (at 5.32892 -3.50012) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at 5.08 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C4-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD8370)
    (at 96.774 104.394 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D814EE)
    (fp_text reference R10 (at 5.32892 -3.50012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at 5.08 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415) (tstamp 57DD8376)
    (at 111.252 104.394 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (path /57D815CB)
    (fp_text reference R11 (at 5.32892 -3.50012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 5.08 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 -1.5) (end 11.4 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.4 -1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.5) (end 11.4 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 -1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 1.27) (end 2.54 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 0) (end 1.27 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.62 0) (end 8.89 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 0) (tstamp 57DD837E)
    (at 129.159 100.711)
    (path /57D8B330)
    (fp_text reference SW1 (at 0 -0.762) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_PUSH (at 0 1.016) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.81 -3.81) (end 3.81 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 -3.81) (end 3.81 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 3.81) (end -3.81 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.81 -3.81) (end -3.81 3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /RESET))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /RESET))
  )

  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 54130A77) (tstamp 57DD838A)
    (at 91.44 129.413)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (path /57D88C5F)
    (fp_text reference U1 (at 0 -5.22) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MCP6002 (at 0 -3.72) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 -2.45) (end -1.4 10.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9 -2.45) (end 9 10.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -2.45) (end 9 -2.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 10.1) (end 9 10.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.135 -2.295) (end 0.135 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.485 -2.295) (end 7.485 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.485 9.915) (end 7.485 8.645) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.135 9.915) (end 0.135 8.645) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.135 -2.295) (end 7.485 -2.295) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.135 9.915) (end 7.485 9.915) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.135 -1.025) (end -1.15 -1.025) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A1))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(R1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(R5-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A0))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 +5V))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C) (tstamp 57DD8460)
    (at 96.52 146.558 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57D819D9)
    (fp_text reference P2 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 1.27) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 4.3) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 1.27) (end -1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A0))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 0) (tstamp 57DD8473)
    (at 116.586 113.411)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57D8755C)
    (fp_text reference P3 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X15 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 37.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 37.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 37.35) (end 1.75 37.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 36.83) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 36.83) (end 1.27 36.83) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 36.83) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P3-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P3-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P3-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P3-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P3-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P3-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P3-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P3-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P3-Pad15)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 0) (tstamp 57DD847E)
    (at 122.364 72.8345)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57D8571B)
    (fp_text reference P4 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X07 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 17) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 17) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 17) (end 1.75 17) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 16.51) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 16.51) (end -1.27 16.51) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 16.51) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /CLK0))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /CLK1))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /CLK2))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /SCL))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /SDA))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 0) (tstamp 57DD8491)
    (at 133.223 113.411)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57D87619)
    (fp_text reference P5 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X15 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 37.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 37.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 37.35) (end 1.75 37.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 36.83) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 36.83) (end 1.27 36.83) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 36.83) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /RESET))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +5V))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P5-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P5-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /SCL))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /SDA))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P5-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(P5-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A1))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A0))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C7-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P5-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P5-Pad15)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0) (tstamp 57DD8498)
    (at 129.159 77.978 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57D853A1)
    (fp_text reference P6 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /CLK0))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (segment (start 122.364 85.5345) (end 122.364 85.0221) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 117.666 85.6615) (end 118.6413 85.6615) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 116.586 121.031) (end 116.586 120.5186) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 116.586 120.5186) (end 116.586 119.8421) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 132.969 98.171) (end 125.349 98.171) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 96.774 104.394) (end 96.774 110.49) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 107.9544 120.5186) (end 106.68 121.793) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 116.586 120.5186) (end 107.9544 120.5186) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 117.666 85.6615) (end 117.666 86.6368) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 133.7476 119.8421) (end 116.586 119.8421) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 134.5763 119.0134) (end 133.7476 119.8421) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 134.5763 117.3043) (end 134.5763 119.0134) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 133.223 115.951) (end 134.5763 117.3043) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 134.5644 99.7664) (end 132.969 98.171) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 134.5644 114.461) (end 134.5644 99.7664) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 134.2633 114.7621) (end 134.5644 114.461) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 133.223 114.7621) (end 134.2633 114.7621) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 133.223 115.951) (end 133.223 114.7621) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 121.3713 98.171) (end 119.8473 96.647) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 125.349 98.171) (end 121.3713 98.171) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 118.872 96.647) (end 119.8473 96.647) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 116.6907 87.6121) (end 117.666 86.6368) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 116.6907 88.9676) (end 116.6907 87.6121) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 119.8473 92.1242) (end 116.6907 88.9676) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 119.8473 96.647) (end 119.8473 92.1242) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 104.521 96.647) (end 96.774 104.394) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 118.872 96.647) (end 104.521 96.647) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 91.186 72.898) (end 90.1076 72.898) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 85.3849 77.6207) (end 90.1076 72.898) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 85.3849 103.0674) (end 85.3849 77.6207) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 95.4474 103.0674) (end 85.3849 103.0674) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 96.774 104.394) (end 95.4474 103.0674) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 91.44 137.033) (end 91.44 135.9077) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 96.774 116.078) (end 96.774 110.49) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 125.389 142.621) (end 126.659 143.891) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 102.6831 142.621) (end 125.389 142.621) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 93.9862 133.9241) (end 102.6831 142.621) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 93.9862 118.8658) (end 93.9862 133.9241) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 96.774 116.078) (end 93.9862 118.8658) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 92.0026 135.9077) (end 91.44 135.9077) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 93.9862 133.9241) (end 92.0026 135.9077) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 129.6791 76.7891) (end 129.159 76.7891) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 130.51 75.9582) (end 129.6791 76.7891) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 130.51 74.249) (end 130.51 75.9582) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 129.159 72.898) (end 130.51 74.249) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 129.159 77.978) (end 129.159 77.3835) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 129.159 77.3835) (end 129.159 76.7891) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 121.0226 79.9142) (end 121.0226 85.0221) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 121.7523 79.1845) (end 121.0226 79.9142) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 127.358 79.1845) (end 121.7523 79.1845) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 129.159 77.3835) (end 127.358 79.1845) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 119.2807 85.0221) (end 121.0226 85.0221) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 118.6413 85.6615) (end 119.2807 85.0221) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 121.0226 85.0221) (end 122.364 85.0221) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 82.677 116.459) (end 82.677 121.793) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 82.296 116.078) (end 82.677 116.459) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 84.328 104.1243) (end 84.328 110.49) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 85.3849 103.0674) (end 84.328 104.1243) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 82.296 113.4973) (end 82.296 116.078) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 84.328 111.4653) (end 82.296 113.4973) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 84.328 110.49) (end 84.328 111.4653) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 91.44 134.493) (end 91.44 133.3677) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 86.828 104.481) (end 86.828 110.49) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 86.741 104.394) (end 86.828 104.481) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 86.868 110.49) (end 92.456 116.078) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 86.828 110.49) (end 86.868 110.49) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 93.419 117.041) (end 92.456 116.078) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 93.419 131.9513) (end 93.419 117.041) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 92.0026 133.3677) (end 93.419 131.9513) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 91.44 133.3677) (end 92.0026 133.3677) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 86.6145 94.1075) (end 86.6145 89.5325) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 86.741 94.234) (end 86.6145 94.1075) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 102.2649 75.057) (end 105.537 75.057) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 87.7894 89.5325) (end 102.2649 75.057) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 86.6145 89.5325) (end 87.7894 89.5325) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 105.5605 72.5805) (end 105.537 72.557) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 112.204 72.5805) (end 105.5605 72.5805) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 104.0337 71.0537) (end 105.537 72.557) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 95.823 71.0537) (end 104.0337 71.0537) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 94.8044 72.0723) (end 95.823 71.0537) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 94.8044 72.898) (end 94.8044 72.0723) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 93.726 72.898) (end 94.8044 72.898) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 97.1225 125.8895) (end 106.934 116.078) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 97.1225 134.5328) (end 97.1225 125.8895) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 98.4974 135.9077) (end 97.1225 134.5328) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 99.06 135.9077) (end 98.4974 135.9077) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 99.06 137.033) (end 99.06 135.9077) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 104.8263 113.9703) (end 106.934 116.078) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 104.8263 110.49) (end 104.8263 113.9703) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 99.274 110.49) (end 104.8263 110.49) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 110.9223 104.394) (end 111.252 104.394) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 104.8263 110.49) (end 110.9223 104.394) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 123.5529 74.0234) (end 122.364 74.0234) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 123.7786 74.2491) (end 123.5529 74.0234) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 129.159 74.2491) (end 123.7786 74.2491) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 129.159 75.438) (end 129.159 74.2491) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 122.364 72.8345) (end 122.364 73.3468) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 122.364 73.3468) (end 122.364 74.0234) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 120.0416 73.3468) (end 119.5293 72.8345) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 122.364 73.3468) (end 120.0416 73.3468) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 118.554 72.8345) (end 119.5293 72.8345) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 107.1245 82.7405) (end 112.204 82.7405) (width 0.25) (layer B.Cu) (net 7))
  (segment (start 116.054 78.8905) (end 116.054 72.8345) (width 0.25) (layer B.Cu) (net 7))
  (segment (start 112.204 82.7405) (end 116.054 78.8905) (width 0.25) (layer B.Cu) (net 7))
  (segment (start 111.252 94.234) (end 111.252 94.147) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 111.2515 94.1465) (end 111.252 94.147) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 111.2515 89.5375) (end 111.2515 94.1465) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 111.252 94.147) (end 118.872 94.147) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 122.364 88.0745) (end 122.364 88.1262) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 117.7013 88.1262) (end 122.364 88.1262) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 117.666 88.1615) (end 117.7013 88.1262) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 102.5067 124.841) (end 99.06 128.2877) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 129.413 124.841) (end 102.5067 124.841) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 132.0341 122.2199) (end 129.413 124.841) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 133.223 122.2199) (end 132.0341 122.2199) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 133.223 121.031) (end 133.223 122.2199) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 99.06 129.413) (end 99.06 128.2877) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 135.0453 119.2087) (end 133.223 121.031) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 135.0453 98.7718) (end 135.0453 119.2087) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 124.3997 88.1262) (end 135.0453 98.7718) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 122.364 88.1262) (end 124.3997 88.1262) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 133.223 143.891) (end 129.159 143.891) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 97.1595 89.5375) (end 96.9645 89.3425) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 101.0915 89.5375) (end 97.1595 89.5375) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 96.9645 82.7405) (end 96.9645 89.3425) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 96.9645 89.3425) (end 96.7745 89.5325) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 96.7745 94.2335) (end 96.7745 89.5325) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 96.774 94.234) (end 96.7745 94.2335) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 97.9883 146.431) (end 97.8613 146.558) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 106.68 146.431) (end 97.9883 146.431) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 96.52 146.558) (end 97.8613 146.558) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 107.188 140.081) (end 99.06 131.953) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 124.2881 140.081) (end 107.188 140.081) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 127.7444 143.5373) (end 124.2881 140.081) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 129.9307 141.351) (end 127.7444 143.5373) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 133.223 141.351) (end 129.9307 141.351) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 107.95 145.161) (end 106.68 146.431) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 126.7762 145.161) (end 107.95 145.161) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 127.7444 144.1928) (end 126.7762 145.161) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 127.7444 143.5373) (end 127.7444 144.1928) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 93.98 146.558) (end 92.6387 146.558) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 95.3214 147.8994) (end 93.98 146.558) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 115.2446 147.8994) (end 95.3214 147.8994) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 115.3881 147.7559) (end 115.2446 147.8994) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 128.4554 147.7559) (end 115.3881 147.7559) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 131.1313 145.08) (end 128.4554 147.7559) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 133.9082 145.08) (end 131.1313 145.08) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 134.5741 144.4141) (end 133.9082 145.08) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 134.5741 140.8309) (end 134.5741 144.4141) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 133.7431 139.9999) (end 134.5741 140.8309) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 133.223 139.9999) (end 133.7431 139.9999) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 133.223 138.811) (end 133.223 139.9999) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 91.44 129.413) (end 91.44 130.5383) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 90.8774 130.5383) (end 91.44 130.5383) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 89.9541 131.4616) (end 90.8774 130.5383) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 89.9541 146.431) (end 89.9541 131.4616) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 82.677 146.431) (end 89.9541 146.431) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 92.5117 146.431) (end 92.6387 146.558) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 89.9541 146.431) (end 92.5117 146.431) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 133.7431 127.4621) (end 133.223 127.4621) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 135.9461 125.2591) (end 133.7431 127.4621) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 135.9461 94.7054) (end 135.9461 125.2591) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 122.8841 81.6434) (end 135.9461 94.7054) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 122.364 81.6434) (end 122.8841 81.6434) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 122.364 80.4545) (end 122.364 81.6434) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 133.223 128.651) (end 133.223 127.4621) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 132.7029 130.0021) (end 133.223 130.0021) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 131.872 129.1712) (end 132.7029 130.0021) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 131.872 125.6065) (end 131.872 129.1712) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 132.6375 124.841) (end 131.872 125.6065) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 133.793 124.841) (end 132.6375 124.841) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 135.4957 123.1383) (end 133.793 124.841) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 135.4957 96.795) (end 135.4957 123.1383) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 122.8841 84.1834) (end 135.4957 96.795) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 122.364 84.1834) (end 122.8841 84.1834) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 122.364 82.9945) (end 122.364 84.1834) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 133.223 131.191) (end 133.223 130.0021) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 133.223 118.491) (end 133.223 117.3021) (width 0.25) (layer B.Cu) (net 33))
  (segment (start 130.7942 103.251) (end 131.8816 104.3384) (width 0.25) (layer B.Cu) (net 33))
  (segment (start 125.349 103.251) (end 130.7942 103.251) (width 0.25) (layer B.Cu) (net 33))
  (segment (start 131.8816 116.4808) (end 131.8816 104.3384) (width 0.25) (layer B.Cu) (net 33))
  (segment (start 132.7029 117.3021) (end 131.8816 116.4808) (width 0.25) (layer B.Cu) (net 33))
  (segment (start 133.223 117.3021) (end 132.7029 117.3021) (width 0.25) (layer B.Cu) (net 33))
  (segment (start 131.8816 104.3384) (end 132.969 103.251) (width 0.25) (layer B.Cu) (net 33))
  (segment (start 82.677 136.271) (end 82.677 131.953) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 86.4081 128.2219) (end 82.677 131.953) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 92.2326 128.2219) (end 86.4081 128.2219) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 92.9687 128.958) (end 92.2326 128.2219) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 92.9687 130.4243) (end 92.9687 128.958) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 91.44 131.953) (end 92.9687 130.4243) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 105.5079 130.7809) (end 106.68 131.953) (width 0.25) (layer B.Cu) (net 41))
  (segment (start 98.2582 130.7809) (end 105.5079 130.7809) (width 0.25) (layer B.Cu) (net 41))
  (segment (start 97.5729 131.4662) (end 98.2582 130.7809) (width 0.25) (layer B.Cu) (net 41))
  (segment (start 97.5729 132.4432) (end 97.5729 131.4662) (width 0.25) (layer B.Cu) (net 41))
  (segment (start 98.4974 133.3677) (end 97.5729 132.4432) (width 0.25) (layer B.Cu) (net 41))
  (segment (start 99.06 133.3677) (end 98.4974 133.3677) (width 0.25) (layer B.Cu) (net 41))
  (segment (start 106.68 136.271) (end 106.68 131.953) (width 0.25) (layer B.Cu) (net 41))
  (segment (start 99.06 134.493) (end 99.06 133.3677) (width 0.25) (layer B.Cu) (net 41))

)
