(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-2~bpo8+1-stable)

  (general
    (links 130)
    (no_connects 130)
    (area 123.956999 89.993 192.560334 117.376333)
    (thickness 1.6)
    (drawings 8)
    (tracks 1)
    (zones 0)
    (modules 51)
    (nets 73)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 /D-)
  (net 5 /D+)
  (net 6 "Net-(P1-Pad4)")
  (net 7 "Net-(P3-Pad1)")
  (net 8 "Net-(P3-Pad2)")
  (net 9 "Net-(P3-Pad3)")
  (net 10 "Net-(P3-Pad4)")
  (net 11 "Net-(P3-Pad5)")
  (net 12 "Net-(P3-Pad6)")
  (net 13 "Net-(P3-Pad7)")
  (net 14 "Net-(P3-Pad8)")
  (net 15 "Net-(P4-Pad1)")
  (net 16 "Net-(P4-Pad2)")
  (net 17 "Net-(P4-Pad3)")
  (net 18 "Net-(P4-Pad4)")
  (net 19 "Net-(P4-Pad5)")
  (net 20 "Net-(P4-Pad6)")
  (net 21 "Net-(P4-Pad7)")
  (net 22 "Net-(P4-Pad8)")
  (net 23 /TxD_RxD)
  (net 24 /RxD_TxD)
  (net 25 /S2)
  (net 26 /S1)
  (net 27 /S0)
  (net 28 "Net-(C8-Pad2)")
  (net 29 "Net-(C9-Pad2)")
  (net 30 "Net-(C17-Pad2)")
  (net 31 "Net-(P1-Pad2)")
  (net 32 "Net-(P1-Pad3)")
  (net 33 /nE)
  (net 34 "Net-(U4-Pad1)")
  (net 35 "Net-(U4-Pad12)")
  (net 36 "Net-(U4-Pad18)")
  (net 37 "Net-(U4-Pad19)")
  (net 38 "Net-(U4-Pad22)")
  (net 39 "Net-(U4-Pad25)")
  (net 40 "Net-(U4-Pad26)")
  (net 41 "Net-(U4-Pad27)")
  (net 42 "Net-(U4-Pad31)")
  (net 43 "Net-(U4-Pad32)")
  (net 44 "Net-(U4-Pad33)")
  (net 45 "Net-(U4-Pad36)")
  (net 46 "Net-(U4-Pad37)")
  (net 47 "Net-(U4-Pad38)")
  (net 48 "Net-(U4-Pad39)")
  (net 49 "Net-(U4-Pad40)")
  (net 50 "Net-(U4-Pad41)")
  (net 51 "Net-(D1-Pad1)")
  (net 52 "Net-(D2-Pad1)")
  (net 53 /LED1)
  (net 54 /LED0)
  (net 55 "Net-(R7-Pad1)")
  (net 56 "Net-(R8-Pad1)")
  (net 57 "Net-(R9-Pad1)")
  (net 58 "Net-(R10-Pad1)")
  (net 59 "Net-(R11-Pad1)")
  (net 60 "Net-(R12-Pad1)")
  (net 61 "Net-(R13-Pad1)")
  (net 62 "Net-(R14-Pad1)")
  (net 63 "Net-(R15-Pad1)")
  (net 64 "Net-(R16-Pad1)")
  (net 65 "Net-(R17-Pad1)")
  (net 66 "Net-(R18-Pad1)")
  (net 67 "Net-(R19-Pad1)")
  (net 68 "Net-(R20-Pad1)")
  (net 69 "Net-(R21-Pad1)")
  (net 70 "Net-(R22-Pad1)")
  (net 71 /RESET)
  (net 72 /MOSI)

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /D+)
    (add_net /D-)
    (add_net /LED0)
    (add_net /LED1)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /RxD_TxD)
    (add_net /S0)
    (add_net /S1)
    (add_net /S2)
    (add_net /TxD_RxD)
    (add_net /nE)
    (add_net GND)
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R22-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad18)")
    (add_net "Net-(U4-Pad19)")
    (add_net "Net-(U4-Pad22)")
    (add_net "Net-(U4-Pad25)")
    (add_net "Net-(U4-Pad26)")
    (add_net "Net-(U4-Pad27)")
    (add_net "Net-(U4-Pad31)")
    (add_net "Net-(U4-Pad32)")
    (add_net "Net-(U4-Pad33)")
    (add_net "Net-(U4-Pad36)")
    (add_net "Net-(U4-Pad37)")
    (add_net "Net-(U4-Pad38)")
    (add_net "Net-(U4-Pad39)")
    (add_net "Net-(U4-Pad40)")
    (add_net "Net-(U4-Pad41)")
  )

  (module Pin_Headers:Pin_Header_Straight_2x03 (layer B.Cu) (tedit 57C1449A) (tstamp 57C14189)
    (at 151.003 110.998 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57C14197)
    (fp_text reference P5 (at -0.889 2.684001 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_02X03 (at 1.27 -7.62 270) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -1.27 -1.27) (end -1.27 -6.35) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.55 1.55) (end 0 1.55) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.75 1.75) (end -1.75 -6.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start 4.3 1.75) (end 4.3 -6.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.75 1.75) (end 4.3 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.75 -6.85) (end 4.3 -6.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 -1.27) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.27 -1.27) (end -1.27 -1.27) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.27 -6.35) (end 3.81 -6.35) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.81 -6.35) (end 3.81 -1.27) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.55 1.55) (end -1.55 0) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.81 1.27) (end 1.27 1.27) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.81 -1.27) (end 3.81 1.27) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.762 0 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 33 /nE))
    (pad 2 smd rect (at 3.302 0 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -0.762 -2.54 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 53 /LED1))
    (pad 4 smd rect (at 3.302 -2.54 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 72 /MOSI))
    (pad 5 smd rect (at -0.762 -5.08 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 71 /RESET))
    (pad 6 smd rect (at 3.302 -5.08 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 579A4441) (tstamp 5789E0C1)
    (at 168.91 108.966 270)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /57C03578)
    (attr smd)
    (fp_text reference U2 (at -4.953 -1.905 540) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 74HCT4051 (at 0 -3.55 270) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -3.95 2.8) (end -3.95 -2.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.95 2.8) (end 3.95 -2.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.95 2.8) (end 3.95 2.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.95 -2.8) (end 3.95 -2.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.2 -2.725) (end 2.2 -2.725) (layer B.SilkS) (width 0.15))
    (fp_line (start -3.775 2.725) (end 2.2 2.725) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.95 2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at -2.95 1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R13-Pad1)"))
    (pad 3 smd rect (at -2.95 0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 23 /TxD_RxD))
    (pad 4 smd rect (at -2.95 0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(R14-Pad1)"))
    (pad 5 smd rect (at -2.95 -0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R12-Pad1)"))
    (pad 6 smd rect (at -2.95 -0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 /nE))
    (pad 7 smd rect (at -2.95 -1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -2.95 -2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.95 -2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 25 /S2))
    (pad 10 smd rect (at 2.95 -1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 26 /S1))
    (pad 11 smd rect (at 2.95 -0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 27 /S0))
    (pad 12 smd rect (at 2.95 -0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(R10-Pad1)"))
    (pad 13 smd rect (at 2.95 0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(R7-Pad1)"))
    (pad 14 smd rect (at 2.95 0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(R8-Pad1)"))
    (pad 15 smd rect (at 2.95 1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R9-Pad1)"))
    (pad 16 smd rect (at 2.95 2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 5791D8EB) (tstamp 5789E075)
    (at 187.452 95.25)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /578802D4)
    (fp_text reference P2 (at 0 -2.6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 1.27) (end -1.27 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 -1.27) (end 1.27 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 19.55) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 19.05) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 5791D926) (tstamp 5789E08D)
    (at 182.372 95.25)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57880227)
    (fp_text reference P4 (at 0 -2.6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 1.27) (end -1.27 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 -1.27) (end 1.27 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 19.55) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 19.05) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P4-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P4-Pad4)"))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P4-Pad5)"))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P4-Pad6)"))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P4-Pad7)"))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module crystal:crystal-EURO_3_5_1_BIGPAD (layer F.Cu) (tedit 579A3DBE) (tstamp 5791C8DC)
    (at 164.973 111.379 180)
    (path /57914290)
    (attr smd)
    (fp_text reference Y1 (at -4.699 1.397 180) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.1016)))
    )
    (fp_text value Crystal_Small (at 1.27 3.175 180) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.1016)))
    )
    (fp_line (start -0.19812 0.49784) (end 0.19812 0.49784) (layer F.SilkS) (width 0.06604))
    (fp_line (start 0.19812 0.49784) (end 0.19812 -0.49784) (layer F.SilkS) (width 0.06604))
    (fp_line (start -0.19812 -0.49784) (end 0.19812 -0.49784) (layer F.SilkS) (width 0.06604))
    (fp_line (start -0.19812 0.49784) (end -0.19812 -0.49784) (layer F.SilkS) (width 0.06604))
    (fp_line (start -2.49936 -1.59766) (end 2.49936 -1.59766) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.49936 -1.59766) (end -2.49936 1.59766) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.49936 1.59766) (end 2.49936 1.59766) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.49936 -1.59766) (end 2.49936 1.59766) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.39878 -0.49784) (end -0.39878 0) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.39878 0) (end -0.39878 0.49784) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.39878 -0.49784) (end 0.39878 0) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.39878 0) (end 0.39878 0.49784) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.99822 0) (end -0.39878 0) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.99822 0) (end -0.99822 0.59944) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.39878 0) (end 0.99822 0) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.99822 0) (end 0.99822 -0.59944) (layer F.SilkS) (width 0.127))
    (fp_circle (center -0.99822 0.79756) (end -1.09728 0.89662) (layer F.SilkS) (width 0.0635))
    (fp_circle (center 0.99822 -0.79756) (end 1.09728 -0.89662) (layer F.SilkS) (width 0.0635))
    (pad 1 smd rect (at -1.84912 1.14808 180) (size 2.54 1.778) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C8-Pad2)"))
    (pad 0 smd rect (at 1.84912 1.14808 180) (size 2.54 1.778) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.84912 -1.14808 180) (size 2.54 1.778) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C9-Pad2)"))
    (pad 0 smd rect (at -1.84912 -1.14808 180) (size 2.54 1.778) (layers F.Cu F.Paste F.Mask))
  )

  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 579A4429) (tstamp 5789E0D5)
    (at 168.91 99.441 270)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /5789E407)
    (attr smd)
    (fp_text reference U3 (at -4.953 -1.905 540) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 74HCT4051 (at 0 -3.55 270) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -3.95 2.8) (end -3.95 -2.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.95 2.8) (end 3.95 -2.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.95 2.8) (end 3.95 2.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.95 -2.8) (end 3.95 -2.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.2 -2.725) (end 2.2 -2.725) (layer B.SilkS) (width 0.15))
    (fp_line (start -3.775 2.725) (end 2.2 2.725) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.95 2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at -2.95 1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(R21-Pad1)"))
    (pad 3 smd rect (at -2.95 0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 24 /RxD_TxD))
    (pad 4 smd rect (at -2.95 0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(R22-Pad1)"))
    (pad 5 smd rect (at -2.95 -0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(R20-Pad1)"))
    (pad 6 smd rect (at -2.95 -0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 /nE))
    (pad 7 smd rect (at -2.95 -1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -2.95 -2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.95 -2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 25 /S2))
    (pad 10 smd rect (at 2.95 -1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 26 /S1))
    (pad 11 smd rect (at 2.95 -0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 27 /S0))
    (pad 12 smd rect (at 2.95 -0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(R18-Pad1)"))
    (pad 13 smd rect (at 2.95 0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(R15-Pad1)"))
    (pad 14 smd rect (at 2.95 0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(R16-Pad1)"))
    (pad 15 smd rect (at 2.95 1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(R17-Pad1)"))
    (pad 16 smd rect (at 2.95 2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 5791D92B) (tstamp 5789E081)
    (at 184.912 95.25)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /578800A6)
    (fp_text reference P3 (at 0 -2.6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 1.27) (end -1.27 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 -1.27) (end 1.27 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 19.55) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 19.05) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P3-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P3-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P3-Pad4)"))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad5)"))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P3-Pad6)"))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P3-Pad7)"))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P3-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Connect:USB_Mini-B (layer F.Cu) (tedit 579A448C) (tstamp 578A65DB)
    (at 129.032 104.14)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (path /578834A3)
    (attr smd)
    (fp_text reference P1 (at 4.064 6.731 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_OTG (at 0 -7.0993) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.85 -5.7) (end 4.85 -5.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.85 -5.7) (end 4.85 5.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.85 5.7) (end -4.85 5.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.85 5.7) (end -4.85 -5.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.59918 -3.85064) (end -3.59918 3.85064) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.59994 -3.85064) (end -4.59994 3.85064) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.59994 3.85064) (end 4.59994 3.85064) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.59994 3.85064) (end 4.59994 -3.85064) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.59994 -3.85064) (end -4.59994 -3.85064) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at 3.44932 -1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 3.44932 -0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 3.44932 0) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 3.44932 0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad4)"))
    (pad 5 smd rect (at 3.44932 1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.35026 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.14884 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.35026 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.14884 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0.8509 -2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.8509 2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5791C25A) (tstamp 57910EE6)
    (at 143.002 95.758)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /579174A9)
    (attr smd)
    (fp_text reference R1 (at 0 -1.778) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22 (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P1-Pad2)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /D-))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5791C25E) (tstamp 57910EEC)
    (at 143.002 99.568)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /579177D4)
    (attr smd)
    (fp_text reference R2 (at 0 -1.778) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22 (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /D+))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5791C21C) (tstamp 57910EF2)
    (at 155.448 110.49 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57912DC2)
    (attr smd)
    (fp_text reference R3 (at 3.175 -0.127 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 71 /RESET))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5791B485) (tstamp 57910EF8)
    (at 150.622 105.918 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57914D9E)
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 33 /nE))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5791C26E) (tstamp 57910F00)
    (at 143.002 107.696)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (path /57910D48)
    (attr smd)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LD1117S33TR (at 0 0.762) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.556 1.524) (end -3.556 4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.556 4.572) (end 3.556 4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.556 4.572) (end 3.556 1.524) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.556 -1.524) (end -3.556 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.556 -2.286) (end -2.032 -4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -4.572) (end 2.032 -4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.032 -4.572) (end 3.556 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.556 -2.286) (end 3.556 -1.524) (layer F.SilkS) (width 0.15))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 5791C28D) (tstamp 5794DD24)
    (at 160.147 101.6)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (path /5791076B)
    (attr smd)
    (fp_text reference U4 (at -5.715 -5.842) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ATMEGA32U4-A (at 0 7.45) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -6.7 -6.7) (end -6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.7 -6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 -6.7) (end 6.7 -6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.175 -5.175) (end -5.175 -4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 5.175 -4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -5.175) (end -4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -4.5) (end -6.45 -4.5) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U4-Pad1)"))
    (pad 2 smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /D-))
    (pad 4 smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /D+))
    (pad 5 smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C17-Pad2)"))
    (pad 7 smd rect (at -5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 8 smd rect (at -5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 54 /LED0))
    (pad 9 smd rect (at -5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 53 /LED1))
    (pad 10 smd rect (at -5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 72 /MOSI))
    (pad 11 smd rect (at -5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /nE))
    (pad 12 smd rect (at -4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U4-Pad12)"))
    (pad 13 smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 71 /RESET))
    (pad 14 smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C9-Pad2)"))
    (pad 17 smd rect (at 0 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C8-Pad2)"))
    (pad 18 smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U4-Pad18)"))
    (pad 19 smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U4-Pad19)"))
    (pad 20 smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 /RxD_TxD))
    (pad 21 smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /TxD_RxD))
    (pad 22 smd rect (at 4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U4-Pad22)"))
    (pad 23 smd rect (at 5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 25 smd rect (at 5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U4-Pad25)"))
    (pad 26 smd rect (at 5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U4-Pad26)"))
    (pad 27 smd rect (at 5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U4-Pad27)"))
    (pad 28 smd rect (at 5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /S2))
    (pad 29 smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /S1))
    (pad 30 smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /S0))
    (pad 31 smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U4-Pad31)"))
    (pad 32 smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U4-Pad32)"))
    (pad 33 smd rect (at 5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U4-Pad33)"))
    (pad 34 smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 35 smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U4-Pad36)"))
    (pad 37 smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U4-Pad37)"))
    (pad 38 smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U4-Pad38)"))
    (pad 39 smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U4-Pad39)"))
    (pad 40 smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U4-Pad40)"))
    (pad 41 smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U4-Pad41)"))
    (pad 42 smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 43 smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 5798ED57) (tstamp 5798ED46)
    (at 130.81 96.52 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (path /5798ED95)
    (attr smd)
    (fp_text reference D1 (at 3.048 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 1.75 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 0.75) (end 1.1 0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.6 -0.75) (end 1.1 -0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 0.15) (end -0.1 -0.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 -0.1) (end -0.25 0.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 -0.35) (end -0.35 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0) (end 0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 0) (end 0 -0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -0.35) (end 0 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0.35) (end -0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.9 -0.95) (end 1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 0.95) (end -1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 0.95) (end -1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 -0.95) (end 1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 5798ED4D) (tstamp 5798ED4C)
    (at 130.81 93.98 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (path /5798F1C0)
    (attr smd)
    (fp_text reference D2 (at 3.048 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 1.75 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 0.75) (end 1.1 0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.6 -0.75) (end 1.1 -0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 0.15) (end -0.1 -0.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 -0.1) (end -0.25 0.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 -0.35) (end -0.35 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0) (end 0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 0) (end 0 -0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -0.35) (end 0 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0.35) (end -0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.9 -0.95) (end 1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 0.95) (end -1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 0.95) (end -1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 -0.95) (end 1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5798ED53) (tstamp 5798ED52)
    (at 135.89 96.52 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5798F712)
    (attr smd)
    (fp_text reference R5 (at -3.302 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220 (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 53 /LED1))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5798ED50) (tstamp 5798ED58)
    (at 135.89 93.98 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5798F803)
    (attr smd)
    (fp_text reference R6 (at -3.302 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220 (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 54 /LED0))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3C6E) (tstamp 579A3C62)
    (at 150.622 98.298 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57915C8A)
    (attr smd)
    (fp_text reference C12 (at 3.81 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3C72) (tstamp 579A3C8A)
    (at 150.622 100.838)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5791899F)
    (attr smd)
    (fp_text reference C17 (at -3.81 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1µ (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3C9D) (tstamp 579A3CCC)
    (at 150.622 103.378)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /579135FA)
    (attr smd)
    (fp_text reference C7 (at -3.302 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3CE2) (tstamp 579A3CF1)
    (at 136.398 101.346 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57894879)
    (attr smd)
    (fp_text reference C1 (at 0 1.778 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4,7u (at 0 2.1 90) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3CF3) (tstamp 579A3D1B)
    (at 136.398 106.934 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /578961B9)
    (attr smd)
    (fp_text reference C4 (at 0 -2.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10n (at 0 2.1 270) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3D1E) (tstamp 579A3D3A)
    (at 140.462 114.046 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57892620)
    (attr smd)
    (fp_text reference C5 (at 0 -1.778 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3D32) (tstamp 579A3D73)
    (at 145.542 114.046 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57892501)
    (attr smd)
    (fp_text reference C6 (at -0.127 -1.668001 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3D52) (tstamp 579A3DA5)
    (at 155.448 113.284 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57913D48)
    (attr smd)
    (fp_text reference C11 (at 3.81 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 71 /RESET))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3D77) (tstamp 579A3DF8)
    (at 159.766 111.252 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57915A7A)
    (attr smd)
    (fp_text reference C13 (at 3.81 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1 270) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3DCE) (tstamp 579A3E6E)
    (at 163.83 115.062 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /579146CD)
    (attr smd)
    (fp_text reference C9 (at -3.302 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22p (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3DC3) (tstamp 579A3EB2)
    (at 169.926 113.792 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5791464E)
    (attr smd)
    (fp_text reference C8 (at 0 1.778 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22p (at 0 2.1 90) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A3E48) (tstamp 579A3F77)
    (at 168.656 103.378 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57915BC5)
    (attr smd)
    (fp_text reference C15 (at 3.937 0.109999 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1 90) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 57C021C4) (tstamp 579A3F95)
    (at 164.084 97.79 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57893092)
    (attr smd)
    (fp_text reference C3 (at 3.429 0 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100n (at 0 -2.1 270) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.3 1) (end 2.3 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end -2.3 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.3 1) (end 2.3 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.85) (end -0.5 0.85) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.85) (end 0.5 -0.85) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 579A3E89) (tstamp 579A3FB3)
    (at 164.084 107.315 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57892EC4)
    (attr smd)
    (fp_text reference C2 (at 3.429 -0.109999 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100n (at 0 -2.1 270) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.3 1) (end 2.3 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end -2.3 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.3 1) (end 2.3 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.85) (end -0.5 0.85) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.85) (end 0.5 -0.85) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A401D) (tstamp 579A406B)
    (at 153.543 93.218 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57915C25)
    (attr smd)
    (fp_text reference C16 (at 3.81 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A4033) (tstamp 579A40D9)
    (at 159.004 93.218 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57916B74)
    (attr smd)
    (fp_text reference C10 (at -3.81 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579A409D) (tstamp 579A417F)
    (at 166.878 93.218)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /57915B48)
    (attr smd)
    (fp_text reference C14 (at 3.81 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57C1413F) (tstamp 57C018CE)
    (at 177.419 95.377)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C01841)
    (attr smd)
    (fp_text reference R7 (at -3.429 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -2.1) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.4 1) (end 2.4 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end -2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.4 1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.6 -0.875) (end -0.6 -0.875) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.6 0.875) (end 0.6 0.875) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(P3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57C14147) (tstamp 57C018D4)
    (at 177.419 97.917)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C04808)
    (attr smd)
    (fp_text reference R8 (at -3.429 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -2.1) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.4 1) (end 2.4 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end -2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.4 1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.6 -0.875) (end -0.6 -0.875) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.6 0.875) (end 0.6 0.875) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(P3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57C14152) (tstamp 57C018DA)
    (at 177.419 100.457)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C048D0)
    (attr smd)
    (fp_text reference R9 (at -3.429 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -2.1) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.4 1) (end 2.4 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end -2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.4 1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.6 -0.875) (end -0.6 -0.875) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.6 0.875) (end 0.6 0.875) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(P3-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57C1415C) (tstamp 57C018E0)
    (at 177.419 102.997)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C0494F)
    (attr smd)
    (fp_text reference R10 (at -3.937 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -2.1) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.4 1) (end 2.4 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end -2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.4 1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.6 -0.875) (end -0.6 -0.875) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.6 0.875) (end 0.6 0.875) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(P3-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57C14164) (tstamp 57C018E6)
    (at 177.419 105.537)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C049D1)
    (attr smd)
    (fp_text reference R11 (at -3.937 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -2.1) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.4 1) (end 2.4 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end -2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.4 1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.6 -0.875) (end -0.6 -0.875) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.6 0.875) (end 0.6 0.875) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(P3-Pad5)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57C1416D) (tstamp 57C018EC)
    (at 177.419 107.95)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C04A56)
    (attr smd)
    (fp_text reference R12 (at -3.937 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -2.1) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.4 1) (end 2.4 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end -2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.4 1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.6 -0.875) (end -0.6 -0.875) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.6 0.875) (end 0.6 0.875) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(P3-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57C14174) (tstamp 57C018F2)
    (at 177.419 110.617)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C04ADE)
    (attr smd)
    (fp_text reference R13 (at -3.937 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -2.1) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.4 1) (end 2.4 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end -2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.4 1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.6 -0.875) (end -0.6 -0.875) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.6 0.875) (end 0.6 0.875) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P3-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57C1417A) (tstamp 57C018F8)
    (at 177.419 113.157)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C04B69)
    (attr smd)
    (fp_text reference R14 (at -3.937 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -2.1) (layer B.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.4 1) (end 2.4 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end -2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.4 1) (end 2.4 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.6 -0.875) (end -0.6 -0.875) (layer B.SilkS) (width 0.15))
    (fp_line (start -0.6 0.875) (end 0.6 0.875) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(R14-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(P3-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57C14142) (tstamp 57C018FE)
    (at 177.419 95.377)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C04E8B)
    (attr smd)
    (fp_text reference R15 (at -3.937 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end -2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57C1414D) (tstamp 57C01904)
    (at 177.419 97.917)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C05322)
    (attr smd)
    (fp_text reference R16 (at -3.937 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end -2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57C14155) (tstamp 57C0190A)
    (at 177.419 100.457)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C053BE)
    (attr smd)
    (fp_text reference R17 (at -3.937 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end -2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R17-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P4-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57C1415F) (tstamp 57C01910)
    (at 177.419 102.997)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C05455)
    (attr smd)
    (fp_text reference R18 (at -3.937 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end -2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R18-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P4-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57C14167) (tstamp 57C01916)
    (at 177.419 105.537)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C054EF)
    (attr smd)
    (fp_text reference R19 (at -3.937 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end -2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P4-Pad5)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57C14170) (tstamp 57C0191C)
    (at 177.419 108.077)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C0558C)
    (attr smd)
    (fp_text reference R20 (at -3.937 -0.127) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end -2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P4-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57C14176) (tstamp 57C01922)
    (at 177.419 110.617)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C0562C)
    (attr smd)
    (fp_text reference R21 (at -3.937 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end -2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R21-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P4-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57C1417E) (tstamp 57C01928)
    (at 177.419 113.157)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /57C056CF)
    (attr smd)
    (fp_text reference R22 (at -3.937 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 2.1) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.4 -1) (end 2.4 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 -1) (end -2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1) (end 2.4 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R22-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P4-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text "RX - TX - GND" (at 185.166 115.824) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (gr_line (start 190.246 116.84) (end 177.8 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190.246 91.44) (end 177.8 91.44) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190.246 91.44) (end 190.246 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "USB2SerialMux v0.2\n08/2016 by Kai Lauterbach\nme@klaute.de - https://klaute.de\n@KaiLauterbach" (at 125.476 113.665 180) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.175)) (justify left mirror))
  )
  (gr_line (start 177.8 116.84) (end 124.46 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.46 91.44) (end 177.8 91.44) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.46 116.84) (end 124.46 91.44) (angle 90) (layer Edge.Cuts) (width 0.1))

  (segment (start 139.212 113.6834) (end 139.212 114.046) (width 0.25) (layer F.Cu) (net 1))

)
