(module 03962A (layer F.Cu) (tedit 5C3915A0)
  (fp_text reference REF** (at 2.3 -0.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 03962A (at 2.3 18.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 27.056963 17.011121) (end 0.056963 17.011121) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.056963 0.011121) (end 27.056963 0.011121) (layer F.SilkS) (width 0.15))
  (fp_line (start 27.056963 0.011121) (end 27.056963 2.011121) (layer F.SilkS) (width 0.15))
  (fp_line (start 27.056963 2.011121) (end 26.056963 3.011121) (layer F.SilkS) (width 0.15))
  (fp_line (start 26.056963 3.011121) (end 26.056963 14.011121) (layer F.SilkS) (width 0.15))
  (fp_line (start 26.056963 14.011121) (end 27.056963 15.011121) (layer F.SilkS) (width 0.15))
  (fp_line (start 27.056963 15.011121) (end 27.056963 17.011121) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.1 6) (end -1.1 12) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.1 12) (end 3.9 12) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.9 12) (end 3.9 5) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.9 5) (end -1.1 5) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.1 5) (end -1.1 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 0) (end 0 5) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 12) (end 0 17) (layer F.SilkS) (width 0.15))
  (fp_text user 03962A (at 15 2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user + (at 3 1.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user - (at 3 15.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user OUT- (at 22 15.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user B- (at 23 13.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user B+ (at 23 3.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user OUT+ (at 22 1.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "Charge here" (at 11.2 8.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6.4 8.4) (end 5 8.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 5 8.4) (end 5.6 8) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.6 8) (end 5 8.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 5 8.4) (end 5.6 8.8) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at 1.4 1.4) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 thru_hole rect (at 24.9 1.4) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 3 thru_hole rect (at 24.9 3.8) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 4 thru_hole rect (at 24.9 13.2) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 5 thru_hole rect (at 24.9 15.6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 6 thru_hole rect (at 1.4 15.6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
