(module APDS-9960 (layer F.Cu) (tedit 5C367739)
  (fp_text reference REF** (at 12.7 15.24) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value APDS-9960 (at 7.62 17.78) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.3 1.44) (end 1.3 16.44) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.3 1.44) (end 21.3 1.44) (layer F.SilkS) (width 0.15))
  (fp_line (start 21.3 1.44) (end 21.3 16.44) (layer F.SilkS) (width 0.15))
  (fp_line (start 21.3 16.44) (end 1.3 16.44) (layer F.SilkS) (width 0.15))
  (fp_text user "VL " (at 5.08 2.54) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at 5.08 5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VCC (at 5.08 7.62) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SDA (at 5.08 10.16) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SCL (at 5.08 12.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user INT (at 5.08 15.24) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user ADPS-9960 (at 18.1 8.4 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.54 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2.54 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 2.54 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 2.54 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 2.54 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
